# mix-calibration Specification

## Purpose

Post-processing calibrator that applies role-aware volume, EQ, stereo width, sends, and mastering chain to a `SongDefinition` before `.rpp` generation.

## Requirements

### Requirement: Calibrator Post-Processing

The system MUST provide a `Calibrator.apply(song: SongDefinition) -> SongDefinition` method that mutates and returns the song with calibrated mix settings. Calibration MUST run as a distinct step between track construction and `RPPBuilder.build()`.

#### Scenario: Happy path — full calibration

- GIVEN a complete `SongDefinition` with 7 tracks (Drumloop, Perc, 808 Bass, Chords, Lead, Clap, Pad) and 2 return tracks
- WHEN `Calibrator.apply(song)` is called
- THEN `song.tracks[].volume` matches role-based LUFS targets
- AND each non-return track has a ReaEQ plugin prepended to its `plugins` list
- AND `song.tracks[].pan` follows stereo-width rules
- AND `song.tracks[].send_level` contains calibrated reverb/delay values
- AND `song.master_plugins` contains Ozone 12 Equalizer, Dynamics, Maximizer

### Requirement: Role-Based Volumes

The system SHALL set track volumes from a preset table keyed by track role (name → role mapping). Volumes MUST be in the REAPER-compatible 0.0–1.0 range.

| Role | Volume | Target |
|------|--------|--------|
| drumloop | 0.85 | kick prominence |
| bass | 0.72 | sub-presence |
| chords | 0.78 | harmonic support |
| lead | 0.78 | melody clarity |
| clap | 0.75 | transient punch |
| pad | 0.68 | ambient depth |
| perc | 0.72 | groove feel |

#### Scenario: Unknown track role

- GIVEN a track with name not matching any preset role
- WHEN calibrated
- THEN the track's volume and pan remain unchanged (preserved as-is)

### Requirement: HPF/LPF EQ per Role

The system SHALL prepend a ReaEQ `PluginDef` to each non-return track's `plugins` list with appropriate HPF or LPF parameters. Bass tracks (808 Bass) SHALL receive LPF. All other tracks SHALL receive HPF.

#### Scenario: HPF on lead/chords/pad tracks

- GIVEN a track named "Chords", "Lead", "Pad", "Clap", "Perc", or "Drumloop"
- WHEN calibrated
- THEN a ReaEQ plugin is inserted at `plugins[0]` with param `0=1` (band enabled), `1=1` (HPF type), `2=200.0` (frequency for melodic) or `2=60.0` (drums)

#### Scenario: LPF on bass track

- GIVEN a track named "808 Bass"
- WHEN calibrated
- THEN a ReaEQ plugin is inserted at `plugins[0]` with param `0=1`, `1=0` (LPF type), `2=300.0` (frequency)

#### Scenario: Return tracks excluded

- GIVEN tracks named "Reverb" or "Delay"
- WHEN calibrated
- THEN no ReaEQ plugin is added (return tracks are skipped)

### Requirement: Stereo Width per Role

The system SHALL set track pan values to role-specific defaults.

| Role | Pan | Rationale |
|------|-----|-----------|
| drumloop | 0.0 | mono center |
| bass | 0.0 | mono sub |
| chords | +0.5 | wide right |
| lead | +0.3 | right-leaning |
| clap | -0.15 | off-center left |
| pad | -0.5 | wide left |
| perc | +0.12 | slight right |

### Requirement: Send Calibration

The system SHALL set `send_level` dict entries for reverb (index=return_track_count) and delay (index=return_track_count+1) on each non-return track.

| Role | Reverb | Delay |
|------|--------|-------|
| drumloop | 0.10 | 0.00 |
| bass | 0.05 | 0.02 |
| chords | 0.30 | 0.10 |
| lead | 0.25 | 0.15 |
| clap | 0.10 | 0.00 |
| pad | 0.40 | 0.20 |
| perc | 0.10 | 0.00 |

### Requirement: Master Chain Upgrade

The system SHALL replace `master_plugins` with `["Ozone_12_Equalizer","Ozone_12_Dynamics","Ozone_12_Maximizer"]`. If registry lookup for any Ozone plugin fails, the system MUST fall back to `["Pro-Q_3","Pro-C_2","Pro-L_2"]`.

### Requirement: Calibration Toggle

The system SHALL support a `--no-calibrate` CLI flag. When passed, `Calibrator.apply()` MUST NOT be called. When omitted (default), calibration MUST run. `SongMeta` MAY include an optional `calibrate: bool` field defaulting to `True`.

#### Scenario: --no-calibrate preserves existing behavior

- GIVEN `compose.py --no-calibrate -o out.rpp`
- WHEN the song is built
- THEN `Calibrator.apply()` is never invoked
- AND the generated `.rpp` matches the pre-calibration baseline
